DH-2010P

Architectural and Engineering Specifications

Version 1.1

(Jan. 28, 2021)

Table of Contents

[1 Manufacturer 3](#_Toc62744507)

[2 General 3](#_Toc62744508)

[2.1 Product Description 3](#_Toc62744509)

[2.2 General Specification 3](#_Toc62744510)

[3 Technical Specification 3](#_Toc62744511)

[3.1 Hardware Specification 3](#_Toc62744512)

[3.2 Network Specifications 3](#_Toc62744513)

[3.3 Power Over Ethernet 3](#_Toc62744514)

[3.4 Electrical Specifications 4](#_Toc62744515)

[3.5 Mechanical Specifications 4](#_Toc62744516)

[3.6 Environmental Specifications 4](#_Toc62744517)

[Version History 5](#_Toc62744518)

# Manufacturer

IDIS Co., Ltd.

IDIS Tower, 344 Pangyo-ro, Bundang-gu, Seongnam-si, Gyeonggi-do, 13493, Korea

Tel: +82 31 723 5400

Fax: +82 31 723 5100

# General

## Product Description

DH-2010P is a PoE switch designed and manufactured by IDIS. The PoE switch provides data transmission and power at the same time to the connected network cameras through Ethernet cables by using PoE-enabled ports without need of a separate power outlet for each network camera and it will reduce the installation costs. Two of service ports are RJ-45 connectors that support 10/100/1000 BASE-T without PoE (Power over Ethernet) function. The other ports are RJ-45 connectors that support 10/100 BASE-T with PoE function.

## General Specification

1. The switch shall support 8 RJ45 connectors at 10/100 BASE-T for service ports.
2. The switch shall support 2 RJ45 connectors at 10/100/1000 BASE-T for Uplink ports.
3. The switch shall support IEEE 802.3af-2003 and IEEE 802.3at-2009 PoE standard.
4. The switch shall support up to 8 IEEE 802.3af PDs(Powered Devices) or 2 IEEE 802.3at PDs.
5. The switch shall support 70W for PSE Power Budget.

# Technical Specification

## Hardware Specification

1. CPU: Embedded MIPS
2. System Memory: 256MB SDRAM, 32M Flash
3. Switching Capacity: 5.6Gbps

## Network Specifications

1. Copper Service Port: 8 RJ-45 Connectors(10/100 BASE-T ports)
2. Copper Uplink Port: 2 RJ-45 Connectors(10/100/1000 BASE-T ports)
3. Optical Uplink Port: N/A

## Power Over Ethernet

1. IEEE 802.3af/at compliant
2. Power to application over Ethernet cabling
3. Central power control for greater network utility
4. PoE alternate B power supply
5. Power feeding over 4/5 & 7/8 data twisted.
6. PoE-supported Network Camera Connection
	1. Up to 8 IEEE 802.3af cameras or 2 IEEE802.3at cameras

## Electrical Specifications

1. Power Supply Equipment power budget: 70W
2. Power Consumption: 90W
3. Power Input: AC100-240V, 2.0~1.0A, 50/60Hz
4. Regulatory Approvals:
	1. Electrical: FCC,CE,KC,UL,CB

## Mechanical Specifications

1. Unit Dimensions (W x H x D): 280mm x 44mm x 180mm (11.0" x 1.7" x 7.1")
2. Unit Weight: 1.35Kg (2.97 lbs.)
3. Weight with Packaging: 2.1Kg (4.63 lbs.)

## Environmental Specifications

1. Operating Temperature: 0°C ~ 40°C (32℉~104℉)
2. Operating Humidity: 10~90%
3. Storage Temperature: -30°C ~ 60°C (-22°F ~ 140°F)

# Version History

|  |  |  |  |
| --- | --- | --- | --- |
| **Version** | **Writer** | **Revision Date** | **Remarks** |
| 1.1 | Daniel Lee | Jan. 28. 2021 | L2 feature unsupported |
| 1.0 | Glen Oh | May. 26. 2018 | Initial Release |